1.2Ghz 3W VTX User Manual

Warm tips: make sure to install antenna before using this video transmitter
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Spec: 

	Frequency
	1.2Ghz frequency, A band, 8 channels

	Operating mode
	key button, Tramp protocol 

	Transmission power
	PIT, 25mW, 800mW, 1600mW, 3000mW

	Antenna connector
	MMCX

	Power input
	9-28VDC

	Current consumption
	1300mA@12VDC@3W

	RF impedance
	50Ω

	Input video impedance
	75Ω

	Input video amplitude
	CVBS 0.8~1.2VP-P

	Video format
	NTSC/PAL

	Dimension(L*W*H)
	53.79mm*27.8mm*13.5mm


Instructions for button operation:

1. Power button(4 shifts): green light indicator, short press for power output change, flash times mean current one, such as flash once for 25mW, flash twice for 800mW, flash three times for 1.6W, flash four times for 3W.
2. Power button: long press 2 seconds to change PIT, green light stays always on means PIT mode.
3. Band/CH button: red light for band, Blue light for CH, short press for CH1-CH8 cycle change.

Wiring：
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Frequency Table：

A band:
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Power output：

	25mW
	800mW
	1.6W
	3W@12V/1300mA


